From aa5e9dc53636e5ae40fc1460c7d3897c2d8588fe Mon Sep 17 00:00:00 2001
From: Yuantian Tang <andy.tang@nxp.com>
Date: Mon, 9 Mar 2020 10:44:54 +0800
Subject: [PATCH] arm64: dts: ls1043a: remove thermal zone 5 from dts

Thermal monitor zone 5 does not exist. So remove it
from dts.

Signed-off-by: Yuantian <andy.tang@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi | 4 ----
 1 file changed, 4 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -919,8 +919,4 @@
 	thermal-zone4 {
 		status = "okay";
 	};
-
-	thermal-zone5 {
-		status = "okay";
-	};
 };
